Each L2L system is different and can include different PVC, tubing, and valve parts. Two key primary plumbing parts include a brass 3-way valve and the union. A typical L2L parts list includes:

|  |
| --- |
| Brass 3-way valve |
| 1" PVC 90 |
| 1" Male Adapter (S x MPT) |
| 1" PVC Male Adapter x Barb |
| 1" PVC Tee |
| 1.5" x 1" Reducing Bushing (S x S) |
| 1.5" PVC Female Adapter (FPT x S) |
| Auto vent |
| 1" PVC 45 |
| Hose Clamp |
| 2-Hole Strap |
| 1" PVC Coupling |
| 1" PVC Pipe, schedule 40 (10 feet) |
| Valve box |
| 1" HDPE Tubing |
| 1/2" HDPE Tubing |
| 1" Barbed Ell |
| 1" Barbed Tee |
| 1"x1/2" Barbed reducing tee |
| 1" Barbed coupling |
| Female hose thread |
| 1" PVC (S x Barb) |
| 1" Ball valve |
| 1/2" Ball valve |